{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["proxmark3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"proxmark3","index":0,"n_rows":61,"n_cols":13,"rows_kept":61,"flags":["formulas_cached_only"]}
["Qty","Reference Designators","Value","Description","Digkey P/N","Price /ea","Extend","SMD","..extend","Fine","..extend","PTH","..extend"]
[20,"C1, C4, C18, C19, C21, C22, C23, C24, C25, C26, C28, C29, C30, C31, C32, C44, C46, C47, C10, C45","33n","capacitor, 0603, X7R, 16V","PCC1756CT-ND",{"v":0.0236,"d":"$0.0236"},{"v":0.472,"d":"$0.47"},1,20,null,0,null,0]
[5,"C2, C3, C6, C7, C14","22p","capacitor, 0603, NP0, 100V","PCC1943CT-ND",{"v":0.043,"d":"$0.0430"},{"v":0.21499999999999997,"d":"$0.22"},1,5,null,0,null,0]
[1,"C5","2n","capacitor, 0603, NP0, 50V","490-1458-1-ND",{"v":0.134,"d":"$0.1340"},{"v":0.134,"d":"$0.13"},1,1,null,0,null,0]
[7,"C8, C11, C12, C16, C39, C42, C43","1n","capacitor, 0603, NP0, 100V","490-3281-1-ND",{"v":0.0567,"d":"$0.0567"},{"v":0.39690000000000003,"d":"$0.40"},1,7,null,0,null,0]
[6,"C13, C17, C20, C36, C40, C41",null,"dnp",null,null,0,null,0,null,0,null,0]
[1,"C15","130p","capacitor, 0603, NP0, 100V","490-1354-1-ND",{"v":0.081,"d":"$0.0810"},{"v":0.081,"d":"$0.08"},1,1,null,0,null,0]
[4,"C9, C27, C33, C34","4u7",null,"PCC2168CT-ND",null,0,1,4,null,0,null,0]
[1,"C35","47p","capacitor, 0603, NP0, 100V","445-2306-1-ND",{"v":0.048,"d":"$0.0480"},{"v":0.048,"d":"$0.05"},1,1,null,0,null,0]
[2,"C37, C38","100u","capacitor, aluminum electrolytic","565-2539-1-ND",{"v":0.217,"d":"$0.2170"},{"v":0.434,"d":"$0.43"},1,2,null,0,null,0]
[2,"D3, D2",null,"diode, BAR18","497-2529-1-ND",{"v":0.3,"d":"$0.3000"},{"v":0.6,"d":"$0.60"},1,2,null,0,null,0]
[2,"D10, D11",null,"diode, zener, 47V","MMBZ5261BLT1OSCT-ND",{"v":0.23,"d":"$0.2300"},{"v":0.46,"d":"$0.46"},1,2,null,0,null,0]
[2,"D1, D7",null,"diode, silicon, 200V","BAS21INCT-ND",{"v":0.173,"d":"$0.1730"},{"v":0.346,"d":"$0.35"},1,2,null,0,null,0]
[1,"D4",null,"LED, yellow","LTST-C190KSKT",{"v":0.11,"d":"$0.1100"},{"v":0.11,"d":"$0.11"},1,1,null,0,null,0]
[1,"D5",null,"LED, green","LTST-C190KGKT",{"v":0.11,"d":"$0.1100"},{"v":0.11,"d":"$0.11"},1,1,null,0,null,0]
[2,"D6, D9",null,"LED, red","LTST-C190CKT",{"v":0.083,"d":"$0.0830"},{"v":0.166,"d":"$0.17"},1,2,null,0,null,0]
[1,"D8",null,"TVS, dual","ESDA6V1L",null,0,1,1,null,0,null,0]
[1,"IC1",null,"FPGA, Spartan II","122-1222-ND",{"v":13.41,"d":"$13.4100"},{"v":13.41,"d":"$13.41"},null,0,1,1,null,0]
[1,"IC2",null,"ARM7 micro","AT91SAM7S256AU001-ND",{"v":14.41,"d":"$14.4100"},{"v":14.41,"d":"$14.41"},null,0,1,1,null,0]
[2,"IC3, IC13",null,"3.3V LDO","425-1714-1-ND",{"v":0.4876,"d":"$0.4876"},{"v":0.9752,"d":"$0.98"},1,2,null,0,null,0]
[1,"IC4",null,"single HCU inverter","TC7SU04FCT-ND",{"v":0.36,"d":"$0.3600"},{"v":0.36,"d":"$0.36"},1,1,null,0,null,0]
[1,"IC5",null,"fast comparator","296-18147-1-ND",{"v":4.95,"d":"$4.9500"},{"v":4.95,"d":"$4.95"},null,0,null,0,null,0]
[1,"IC6",null,"10 MHz GBW opamp","MCP6294-E/ST-ND",{"v":2.33,"d":"$2.3300"},{"v":2.33,"d":"$2.33"},1,1,null,0,null,0]
[1,"IC7",null,"reset monitor","MCP100T-300I/TTCT-ND",{"v":0.36,"d":"$0.3600"},{"v":0.36,"d":"$0.36"},1,1,null,0,null,0]
[1,"IC8",null,"fast A/D","296-2184-5-ND",{"v":5.56,"d":"$5.5600"},{"v":5.56,"d":"$5.56"},1,1,null,0,null,0]
[2,"IC9, IC10",null,"74ACT244 buffers","296-1071-1-ND",{"v":0.52,"d":"$0.5200"},{"v":1.04,"d":"$1.04"},1,2,null,0,null,0]
[1,"IC11",null,"CD4066 analog switches","296-14123-1-ND",{"v":0.55,"d":"$0.5500"},{"v":0.55,"d":"$0.55"},1,1,null,0,null,0]
[1,"IC12",null,"2.5V LDO","LP2989IM-2.5-ND",{"v":2.42,"d":"$2.4200"},{"v":2.42,"d":"$2.42"},1,1,null,0,null,0]
[1,"IC14",null,"very fast opamp","AD8052ARM-ND",{"v":3.65,"d":"$3.6500"},{"v":3.65,"d":"$3.65"},1,1,null,0,null,0]
[1,"Q1",null,"2N3904-like NPN","568-1741-1-ND",{"v":0.08,"d":"$0.0800"},{"v":0.08,"d":"$0.08"},1,1,null,0,null,0]
[1,"Q2",null,"dnp","IRF7307-ND",{"v":0.7,"d":"$0.7000"},{"v":0.7,"d":"$0.70"},null,0,null,0,null,0]
[2,"R1, R42","1meg","resistor, 0603, 1%","RHM1.00MHCT-ND",{"v":0.076,"d":"$0.0760"},{"v":0.152,"d":"$0.15"},1,2,null,0,null,0]
[3,"R2, R52, R54",100,"resistor, 0603, 1%","311-100HRCT-ND",{"v":0.077,"d":"$0.0770"},{"v":0.23099999999999998,"d":"$0.23"},1,3,null,0,null,0]
[6,"R3, R53, R24, R25, R26, R55",330,"resistor, 0603, 1%","311-330HRCT-ND",{"v":0.077,"d":"$0.0770"},{"v":0.46199999999999997,"d":"$0.46"},1,6,null,0,null,0]
[2,"R4, R5",27,"resistor, 0603, 1%","311-27.0HRCT-ND",{"v":0.077,"d":"$0.0770"},{"v":0.154,"d":"$0.15"},1,2,null,0,null,0]
[1,"R6","1k5","resistor, 0603, 1%","311-1.50KHRCT-ND",{"v":0.077,"d":"$0.0770"},{"v":0.077,"d":"$0.08"},1,1,null,0,null,0]
[14,"R7, R8, R13, R14, R15, R17, R18, R19, R34, R40, R47, R50, R56, R57","10k","resistor, 0603, 1%","311-10.0KHRCT-ND",{"v":0.077,"d":"$0.0770"},{"v":1.078,"d":"$1.08"},1,14,null,0,null,0]
[3,"R9, R10, R12","100k","resistor, 0603, 1%","311-100KHRCT-ND",{"v":0.077,"d":"$0.0770"},{"v":0.23099999999999998,"d":"$0.23"},1,3,null,0,null,0]
[1,"R11","510k","resistor, 0603, 1%","311-510KHRCT-ND",{"v":0.077,"d":"$0.0770"},{"v":0.077,"d":"$0.08"},1,1,null,0,null,0]
[4,"R16, R32, R35, R58","zerohm","resistor, 0603",null,null,0,1,4,null,0,null,0]
[2,"R20, R31","240k","resistor, 0603, 1%","311-240KHRCT-ND",{"v":0.077,"d":"$0.0770"},{"v":0.154,"d":"$0.15"},1,2,null,0,null,0]
[1,"R21","24k","resistor, 0603, 1%","311-24.0KHRCT-ND",{"v":0.077,"d":"$0.0770"},{"v":0.077,"d":"$0.08"},1,1,null,0,null,0]
[2,"R45, R46","10k","resistor, 0603, 1%",{"$nulls":6},0,null,0]
[4,"R22, R27, R28, R29, R45, R46",33,"resistor, 0603, 1%",null,null,0,null,0,null,0,null,0]
[4,"R23, R39, R43, R44","1k","resistor, 0603, 1%","311-1.00KHRCT-ND",{"v":0.077,"d":"$0.0770"},{"v":0.308,"d":"$0.31"},1,4,null,0,null,0]
[2,"R30, R41","10meg","resistor, 0603, 1%","311-10.0MHRCT-ND",{"v":0.077,"d":"$0.0770"},{"v":0.154,"d":"$0.15"},1,2,null,0,null,0]
[3,"R33, R49, R51","2k4","resistor, 0603, 1%","311-2.40KHRCT-ND",{"v":0.077,"d":"$0.0770"},{"v":0.23099999999999998,"d":"$0.23"},1,3,null,0,null,0]
[4,"R36, R37, R38, R48",null,"dnp",null,null,0,null,0,null,0,null,0]
[1,"R59","3k3","resistor, 0603, 1%","311-3.30KHRCT-ND",{"v":0.077,"d":"$0.0770"},{"v":0.077,"d":"$0.08"},1,1,null,0,null,0]
[1,"RLY1",null,"relay, SMD","(from Newark)",{"v":3.01,"d":"$3.0100"},{"v":3.01,"d":"$3.01"},1,1,null,0,null,0]
[1,"SV1",null,"USB mini-B connector, SMD","H2959CT-ND",{"v":1.39,"d":"$1.3900"},{"v":1.39,"d":"$1.39"},1,1,null,0,null,0]
[1,"SV2",null,"hirose mq172 SMD connector","H2794-ND",{"v":2.13,"d":"$2.1300"},{"v":2.13,"d":"$2.13"},1,1,null,0,null,0]
[1,"SV3",null,"header, 0.100\", 10x2, shrouded","A26273-ND",{"v":1.78,"d":"$1.7800"},{"v":1.78,"d":"$1.78"},null,0,null,0,1,1]
[1,"SV5",null,"dnp",null,null,0,null,0,null,0,null,0]
[1,"SW1",null,"pushbutton","P12969SCT-ND",{"v":1.138,"d":"$1.1380"},{"v":1.138,"d":"$1.14"},1,1,null,0,null,0]
[7,"TP1, TP2, TP3, TP4, TP5, TP7, TP8",null,"test point, SMD","5015KCT-ND",{"v":0.246,"d":"$0.2460"},{"v":1.722,"d":"$1.72"},1,7,null,0,null,0]
[1,"TP6",null,"test point, PTH","5011K-ND",{"v":0.234,"d":"$0.2340"},{"v":0.234,"d":"$0.23"},null,0,null,0,1,1]
[1,"U1",null,"ferrite, 0805","445-1566-1-ND",{"v":0.067,"d":"$0.0670"},{"v":0.067,"d":"$0.07"},1,1,null,0,null,0]
[1,"XT1","13.56 MHz","crystal","(from Newark)",{"v":1.1013,"d":"$1.1013"},{"v":1.1013,"d":"$1.10"},1,1,null,0,null,0]
[1,"XT2","16 MHz","crystal","300-8096-1-ND",{"v":1.1013,"d":"$1.1013"},{"v":1.1013,"d":"$1.10"},1,1,null,0,null,0]
[150,{"$nulls":5},{"v":71.50469999999999,"d":"$71.50"},null,127,null,2,null,2]